2025 – 05 – 19
Updated Joinery, as per client.

PROJECT:	G&I – Office Block

1. Kitchenette area behind the Boardroom TV wall:
· 4630 (L) x 550 (D) x 900 (H) – Height includes base height
· 100mm (H) x 20mm (T) Eezi Qaurtz splash back  – Magnolia
· 20mm Thick Eezi Qaurtz countertop  – Magnolia
· Black grab handle – Length 200mm
· 16mm Melamine framed with impact edging
· Melamine to be Storm Grey 
· 100mm (H) Base to be plywood and covered with Super Black.
· 4x drawers
· 1 x single center shelf in the middle of the cupboards. (Spaces: Top & Bottom)
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2. Server area in kitchenette area behind boardroom TV wall:
· 2065 (L) x 350 (D) x 900 (H) – Height includes base height
· 100mm (H) x 20mm (T) Eezi Qaurtz splash back  – Magnolia
· 20mm Thick Eezi Qaurtz countertop  – Magnolia
· Black grab handle – Length 200mm
· 16mm Melamine framed with impact edging - Dunblane
· Melamine doors - Dunblane 
· 100mm (H) Base to be plywood and covered with Iceberg White.
· 1 x single center shelf in the middle of the cupboards. (Spaces: Top & Bottom)
· Floating shelf:
· 3 x black L-brackets fixed to drywall.
· 32mm (T) melamine with impact edging.
· Colour to be Brookhill Fusion
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3. Boardroom Table:
· 4000 (L) x 1200 (D) x 770 (H) – Height includes base height
· 50mm build up with 16mm Melamine and covered with Oak veneer to match wallpaper wall. 
· 20mm solid oak edging
· 50mm x 70mm powder coated black steel base
· Power docking allowance -  PC of R 4000.00
[image: ]

4. 1 x Slatted  Bench:
· Solid oak slats as per design 
· Mild steel sub frame
[image: A drawing of a bench
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5. Sanding down of wall panels in Boardroom + The frame and backing of the wallpaper:
· Mural Frame: 5450 (L) x 1970 (H) 
· 16mm Backing for wallpaper
· 32mm x 32mm MFD frame around backboard
· 150mm (H) skimmed bulkhead to hide existing sprinkler system piping.
· Painting and sanding of current wall panels (E.g.  panel size - 600x 2320mm)
(Needs to match boardroom table, else we need to make the wall panels oak veneer. As per our discussion.)
[image: ]
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6. Arch wall – Display area:
· 200mm high skimmed bulkhead
· Arch cover panel 18mm shutter-ply (2630mm (H) x 4151 mm (arched length))
· 150mm (H) shutter-ply base + Painted/Sprayed (Either or)
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7. Exhibition space (Display) – VOIDED
PC = R 8200
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8. Kitchenette on First Floor: 
· Replace doors, draw fronts (Re-using existing carcasses only)
· Install new hinges and runners 
· Install new base cladding 
· Black grab handle – Length 200mm
· Remedial repair work to existing cabinets
· Install Eezi quarts 20mm top -  Magnolia
· 4 x floating shelves:
· 1380mm (L) x 300mm (D) x 32mm (H)
· 32mm thick (16x2mm) melamine with matching impact edging.
· Colour to be Brookhill Fusion
2025 – 05 -06 
As per meeting on site with client. It was asked to use the existing carcass as a template to install a complete new kitchenette.
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Please include:  New framed area for wallpaper at bench 
2140mm (w) x 1580mm (h) - To match boardroom frame style and colour.
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