COVERAGE DEFINITION:

'Coverage' means the total percentage of site area that may be covered by buildings, measured over the outside walls and covered by a roof or projection provided that:
(i) the following are to be included in coverage:-
(a) external staircases;
(b) fire escapes;
(c) electrical substations for the exclusive use of the development;
(d) motor car ramps, the undersides of which are more than 1,5 m above the ground level of
such ramps;
(e) canopies and permanent awnings projecting more than 1 m beyond the building;
(f) canopies over fuel pumps at filling stations/service stations/public garages;
(ii) the following are to be excluded from coverage:-
(a) the area covered by a maximum eaves projection of 1 m;
(b) unroofed stoeps, terraces and patios;
(c) arcade passageways, i.e. any covered walk providing public access, with shops along one or
both sides which are roofed but not built over;
(d) motor car ramps, the undersides of which are 1,5 m or less above the ground level of such
ramps;
(e) basements;
(f) unroofed entrance steps and landings;
(g) minor decorative projections projecting not more than 0,3 m from the wall of such building;
(h) canopies for pedestrian protection at the ground floor of shopping centres;
(i) driveways covered by canopies, whether cantilevered or not, for public protection from the
elements relating to hotels, flats and public buildings and includes a portŠ-cochere;
(j) covered refuse bin storage areas.





FLOOR AREA DEFINITION:

'Floor Area' of a building includes the terms "Gross Leasable Area", "Gross Floor Area", "Gross Building
Area", "Permissible Floor Space" and any other similar term and means the sum total of all floors at all
levels measured over the main containing walls of the building (i.e. outer plinth area of the building) but
shall exclude:-
(a) vertical ventilation shafts, ducts;
(b) lift shafts, staircases;
(c) lift motor rooms and air-conditioning plant rooms;
(d) electricity sub-station/transformer rooms;
(e) the area covered by the projection of the eaves;
(f) any floor area used solely for parking or loading/unloading;
(g) refuse bin storage areas;
(h) unroofed balconies, unroofed terraces;
(i) malls which allow free public access to shops, other buildings, public transport systems or
streets (malls do not include access corridors or foyers);
(j) public or private toilets, staff change rooms, cleaners' and maintenance staff rooms, sick bays;

FLOOR SPACE INDEX (F.S.I.) DEFINITION:

'Floor Space Index' (F.S.I.) includes the terms 'Bulk', 'Floor Area Ratio' and any other similar term and
means the ratio obtained by dividing the floor area by the erf area less any area required for road
widening and for public purposes.
