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Eaves Construction: c;l
80x125mm Aluminium Ogee Gutter Fixed To Fall To
10x250mm Nutech Fibre Cement Fascia
6mm Nutech Fibre Cement Cladding Butt Jointed Between UPVC H
38x50mm Brandering Fixed To Underside Roof Trusses

80mm @ PVC Rainwater Pipe
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75mm BRICK + 10mm JOINT = 85mm BRI

102.475 = UnderSide Slab
Plaster and Paint Finish External Finish As Per Architects Spec.
Exposed Hardwood Timber Staircase Fixed To Galv Steel Centre Spi

270mm Caverty Wall In Stretcher Bond To Have Galv. Wire Ties At
DPC Min 150mm AFGL
Weep Holes Kept Open At Every 5th Perp End
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