HINTERVELD  - 2025/05/05
PAINT COLOURS:
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1. SPA BLUE (Top half of gable and feature colours at Main entrance)
2. CHELSEA FOG (Main external colour)
3. BRILLIANT WHITE (Window bands, eaves, fascia’s, barge boards.
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1. SPA BLUE (Top half of gable and feature colours at Main entrance)
2. CHELSEA FOG (Main external colour)
3. BRILLIANT WHITE (Window bands, eaves, fascia’s, barge boards.)







RECEPTION:
1. SPA BLUE (Feature colour in passage on both sides of the wall.)
2. BRILLIANT WHITE (Ceilings, Cornices, Door frames, Skirtings)
3. DARKEN PUDDLE (Feature wall to be a specialist screeded finish. I will get back to you on this one.)
4. KITTEN WHITE (General internal wall colour)
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PASSAGE 1:
1. KITTEN WHITE (General internal wall colour)
2. BRILLIANT WHITE (Ceilings, Cornices, Door frames, Skirtings)
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OFFICE 1:
All internal walls to be Kitten white.
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Daniels Office:
All internal walls to be Kitten White
[image: A room with a table and chairs

AI-generated content may be incorrect.]

OFFICE 2:
All internal walls to be Kitten white.
[image: A room with computers and chairs

AI-generated content may be incorrect.]

SERVER ROOM:
All internal walls to be Kitten white.
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PASSAGE 1:
1. BRILLIANT WHITE (Ceilings, Cornices, Doors & Door frames, Skirtings)
2. KITTEN WHITE (General internal wall colour)
[image: A white wall with a wood floor
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SHOW ROOM:
1. BRILLIANT WHITE (Ceilings, Cornices, Doors & Door frames, Skirtings)
2. KITTEN WHITE (General internal wall colour)
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COFFEE NOOK:
1. SPA BLUE (Feature colour in passage on both sides of the wall.)
2. BRILLIANT WHITE (Ceilings, Cornices, Doors & Door frames, Skirtings)
3. KITTEN WHITE (General internal wall colour)
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STAFF MALE & FEMALE RESTROOMS:
1. SPA BLUE (Feature colour in passage on both sides of the wall.)
2. BRILLIANT WHITE (Doors, Door frames & Skirtings)
3. KITTEN WHITE (General internal wall colour)3
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CANTEEN:
1. SPA BLUE (Feature colour in passage on both sides of the wall.)
2. BRILLIANT WHITE (Doors, Door frames & Skirtings)
3. KITTEN WHITE (General internal wall colour)
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VISITORS RESTROOM:

1. SPA BLUE (Feature colour in passage on both sides of the wall.)
2. BRILLIANT WHITE (Doors, Door frames & Skirtings)
3. KITTEN WHITE (General internal wall colour)
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GENERAL COMMENTS:
All restrooms to be a 100mm high tiled skirting with L-trim on the top.

Where the urinal has been mounted. The wall tile/skirting will be 150mm above the top side of the push plate. (As per the image below)
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